(kicad_symbol_lib
	(version 20251024)
	(generator "kicad_symbol_editor")
	(generator_version "10.0")
	(symbol "MSPM0G3507SPTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "U"
			(at 1.016 1.27 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MSPM0G3507SPTR"
			(at 29.464 1.27 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 58.928 -68.326 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/mspm0g3507.pdf?ts=1774523228276&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FMSPM0G3507%252Fpart-details%252FMSPM0G3507SRHBR"
			(at 133.604 -71.12 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Microcontroller Cortex-M0+ Arm 80MHz with 128KB flash 32KB SRAM"
			(at 72.898 -65.786 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 47.498 -61.468 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Part Number" "MSPM0G3507SPTR"
			(at 47.498 -63.5 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Distributer Link 1" "https://www.mouser.de/ProductDetail/Texas-Instruments/MSPM0G3507SPTR?qs=ST9lo4GX8V1GEI0H4GAJcA%3D%3D"
			(at 94.742 -80.01 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Distributer Link 2" "https://www.digikey.de/de/products/detail/texas-instruments/MSPM0G3507SPTR/22106901?s=N4IgTCBcDaILIGUAKcAMBxAzAVlQdmQBUAlEAXQF8g"
			(at 109.982 -77.724 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C22362630"
			(at 44.45 -75.692 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "MSPM0G3507SPTR_0_0"
			(pin bidirectional line
				(at -2.54 -3.81 0)
				(length 2.54)
				(name "PA0/FCC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -6.35 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -74.93 0)
				(length 2.54)
				(name "PA28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 40.64 -55.88 180)
				(length 2.54)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 2.54 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -6.35 180)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -8.89 180)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -24.13 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -31.75 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -11.43 180)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -13.97 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -16.51 180)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -19.05 180)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -21.59 180)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -24.13 180)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -26.67 180)
				(length 2.54)
				(name "PB16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -36.83 0)
				(length 2.54)
				(name "PA13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "MSPM0G3507SPTR_1_0"
			(pin bidirectional line
				(at -2.54 -77.47 0)
				(length 2.54)
				(name "PA31/CLK_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 21.59 -83.82 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -8.89 0)
				(length 2.54)
				(name "PA2/ROSC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -11.43 0)
				(length 2.54)
				(name "PA3/COMP1_OUT/LFXIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -13.97 0)
				(length 2.54)
				(name "PA4/LFCLK_IN/LFX_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -16.51 0)
				(length 2.54)
				(name "PA5/HFXIN/FCC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -19.05 0)
				(length 2.54)
				(name "PA6/HFCLK_IN/HFXOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -21.59 0)
				(length 2.54)
				(name "PA7/CLK_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -26.67 0)
				(length 2.54)
				(name "PA9/RTC_OUT/CLK_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -29.21 0)
				(length 2.54)
				(name "PA10/CLK_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -34.29 0)
				(length 2.54)
				(name "PA12/FCC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -39.37 0)
				(length 2.54)
				(name "PA14/CLK_OUT/A0_12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -41.91 0)
				(length 2.54)
				(name "PA15/A1_0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -44.45 0)
				(length 2.54)
				(name "PA16/A1_1/FCC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -46.99 0)
				(length 2.54)
				(name "PA17/A1_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -49.53 0)
				(length 2.54)
				(name "PA18/A1_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -52.07 0)
				(length 2.54)
				(name "PA19/SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -54.61 0)
				(length 2.54)
				(name "PA20/SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -29.21 180)
				(length 2.54)
				(name "PB17/A1_4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -31.75 180)
				(length 2.54)
				(name "PB18/A1_5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -34.29 180)
				(length 2.54)
				(name "PB19/A1_6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -57.15 0)
				(length 2.54)
				(name "PA21/A1_7/VREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -59.69 0)
				(length 2.54)
				(name "PA22/CLK_OUT/A0_7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -36.83 180)
				(length 2.54)
				(name "PB20/A0_6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 40.64 -39.37 180)
				(length 2.54)
				(name "PB24/A0_5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -62.23 0)
				(length 2.54)
				(name "PA23/VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -64.77 0)
				(length 2.54)
				(name "PA24/A0_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -67.31 0)
				(length 2.54)
				(name "PA25/A0_2/OPA0_IN1+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -69.85 0)
				(length 2.54)
				(name "PA26/A0_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -72.39 0)
				(length 2.54)
				(name "PA27/RTC_OUT/A0_0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 19.05 2.54 270)
				(length 2.54)
				(name "VCORE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "MSPM0G3507SPTR_1_1"
			(rectangle
				(start 0 0)
				(end 38.1 -81.28)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(text "Texas\nInstruments\nMSPM0G3507\nLQFP - 48"
				(at 31.496 -76.2 0)
				(effects
					(font
						(face "Adwaita Sans")
						(size 1.27 1.27)
						(thickness 0.254)
						(bold yes)
						(color 0 0 72 1)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
